(footprint "WLCSP-71_9x8_4.062x3.762mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Baochip0 WLCSP footprint")
	(property "Reference" "REF**"
		(at 0 -2.881 0)
		(layer "F.SilkS")
	)
	(property "Value" "WLCSP-72_9x8_4.062x3.762mm"
		(at 0 2.881 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "Baochip0 footprint"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A2" smd circle
		(at -1.2 -1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -0.8 -1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -0.4 -1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at 0 -1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at 0.4 -1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at 0.8 -1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 1.2 -1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 1.6 -1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -1.6 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -1.2 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -0.8 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -0.4 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at 0 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at 0.4 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at 0.8 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 1.2 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 1.6 -1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -1.6 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -1.2 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -0.8 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -0.4 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at 0 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at 0.4 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at 0.8 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 1.2 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at 1.6 -0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -1.6 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -1.2 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -0.8 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -0.4 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at 0 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at 0.4 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at 0.8 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 1.2 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 1.6 -0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -1.6 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -1.2 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -0.8 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -0.4 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at 0 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at 0.4 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at 0.8 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 1.2 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at 1.6 0.2)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -1.6 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -1.2 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -0.8 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -0.4 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at 0 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at 0.4 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at 0.8 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 1.2 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at 1.6 0.6)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -1.6 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -1.2 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -0.8 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -0.4 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at 0 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at 0.4 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at 0.8 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 1.2 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 1.6 1)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -1.6 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -1.2 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -0.8 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -0.4 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at 0 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at 0.4 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at 0.8 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 1.2 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 1.6 1.4)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "F:/largework/kicad/common/baochip0-es.STEP"
		(offset (xyz 0 0 0.46))
		(scale (xyz 1 1 1))
		(rotate (xyz -0 -180 -0))
	)
)
