(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "baochip1x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.254 1.524 0)
		)
		(property "Value" "baochip1x"
			(at 0.254 1.524 0)
		)
		(property "Footprint" "common:WLCSP-71_9x8_4.062x3.762mm"
			(at 0.254 1.524 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Baochip0 WLCSP"
			(at 0.254 1.524 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "baochip1x_1_1"
			(pin power_in line
				(at -12.7 -3.81 0)
				(length 2.54)
				(name "V3.3IN")
				(number "A3")
			)
			(pin power_in line
				(at -12.7 -6.35 0)
				(length 2.54)
				(name "V3.3RR")
				(number "H4")
			)
			(pin power_in line
				(at -12.7 -11.43 0)
				(length 2.54)
				(name "VDDIO")
				(number "B7")
			)
			(pin power_in line
				(at -12.7 -13.97 0)
				(length 2.54)
				(name "VDDIO")
				(number "C7")
			)
			(pin power_in line
				(at -12.7 -16.51 0)
				(length 2.54)
				(name "VDDAO")
				(number "E6")
			)
			(pin power_in line
				(at -12.7 -21.59 0)
				(length 2.54)
				(name "VDD2.5")
				(number "C1")
			)
			(pin power_in line
				(at -12.7 -26.67 0)
				(length 2.54)
				(name "VDD.85")
				(number "A4")
			)
			(pin power_in line
				(at -12.7 -29.21 0)
				(length 2.54)
				(name "VDD.85")
				(number "E7")
			)
			(pin power_in line
				(at -12.7 -31.75 0)
				(length 2.54)
				(name "VDD.85")
				(number "F7")
			)
			(pin power_in line
				(at 10.16 -16.51 180)
				(length 2.54)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at 10.16 -19.05 180)
				(length 2.54)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at 10.16 -21.59 180)
				(length 2.54)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at 10.16 -24.13 180)
				(length 2.54)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at 10.16 -26.67 180)
				(length 2.54)
				(name "GND")
				(number "B2")
			)
			(pin input line
				(at 10.16 -31.75 180)
				(length 2.54)
				(name "GND_TP")
				(number "D5")
			)
		)
		(symbol "baochip1x_2_1"
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "USB_D+")
				(number "A2")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "USB_D-")
				(number "B1")
			)
			(pin input inverted
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "XRSTn")
				(number "E5")
			)
			(pin input inverted
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "AORSTn")
				(number "H5")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "X32KIN")
				(number "B3")
			)
			(pin output line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "X32KOUT")
				(number "B4")
			)
			(pin input line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "X48MI")
				(number "H1")
			)
			(pin output line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "X48MO")
				(number "H2")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "DUART")
				(number "D3")
			)
		)
		(symbol "baochip1x_3_1"
			(text "GPIO"
				(at -7.112 -3.048 0)
			)
			(text "AF1      AF2      AF3      BIO\nCAMD[0]           PWM_1[0] 0\nCAMD[1]           PWM_1[1] 1\nCAMD[2]           PWM_1[2] 2\nCAMD[3]           PWM_1[3] 3\nCAMD[4]                    4\nCAMD[5]                    5\nCAMD[6]                    6\nCAMD[7]                    7\nCAM_HS   SPMCLK_2          8\nCAM_VS   SPMD0_2           9\nCAM_CK   SPMD1_2           10\nI2CSCL_0 SPMCS0_2          11\nI2CSDA_0 SPMCS1_2          12\nUARTRX_2 SCIF_SCK          13\nUARTTX_2 SCIF_DAT          14\n                           15"
				(at -0.762 -3.048 0)
			)
			(pin bidirectional line
				(at -10.16 -6.35 0)
				(length 2.54)
				(name "PB0")
				(number "D6")
			)
			(pin bidirectional line
				(at -10.16 -8.89 0)
				(length 2.54)
				(name "PB1")
				(number "A9")
			)
			(pin bidirectional line
				(at -10.16 -11.43 0)
				(length 2.54)
				(name "PB2")
				(number "A8")
			)
			(pin bidirectional line
				(at -10.16 -13.97 0)
				(length 2.54)
				(name "PB3")
				(number "A7")
			)
			(pin bidirectional line
				(at -10.16 -16.51 0)
				(length 2.54)
				(name "PB4")
				(number "A6")
			)
			(pin bidirectional line
				(at -10.16 -19.05 0)
				(length 2.54)
				(name "PB5")
				(number "A5")
			)
			(pin bidirectional line
				(at -10.16 -21.59 0)
				(length 2.54)
				(name "PB6")
				(number "B5")
			)
			(pin bidirectional line
				(at -10.16 -24.13 0)
				(length 2.54)
				(name "PB7")
				(number "B6")
			)
			(pin bidirectional line
				(at -10.16 -26.67 0)
				(length 2.54)
				(name "PB8")
				(number "B8")
			)
			(pin bidirectional line
				(at -10.16 -29.21 0)
				(length 2.54)
				(name "PB9")
				(number "C8")
			)
			(pin bidirectional line
				(at -10.16 -31.75 0)
				(length 2.54)
				(name "PB10")
				(number "D8")
			)
			(pin bidirectional line
				(at -10.16 -34.29 0)
				(length 2.54)
				(name "PB11")
				(number "B9")
			)
			(pin bidirectional line
				(at -10.16 -36.83 0)
				(length 2.54)
				(name "PB12")
				(number "C9")
			)
			(pin bidirectional line
				(at -10.16 -39.37 0)
				(length 2.54)
				(name "PB13")
				(number "D9")
			)
			(pin bidirectional line
				(at -10.16 -41.91 0)
				(length 2.54)
				(name "PB14")
				(number "E9")
			)
			(pin bidirectional line
				(at -10.16 -44.45 0)
				(length 2.54)
				(name "PB15")
				(number "G6")
			)
		)
		(symbol "baochip1x_4_1"
			(text "GPIO"
				(at -7.112 -3.048 0)
			)
			(text "AF1      AF2      AF3      BIO\nSDIOCLK  SPMCLK_2 PWM_2[0] 16\nSDIOCMD  SPMD0_2  PWM_2[1] 17\nSDIOD0   SPMD1_2  PWM_2[2] 18\nSDIOD1   SPMCS0_2 PWM_2[3] 19\nSDIOD2   SPMCS1_2          20\nSDIOD3   I2CSCL_3          21\n         I2CSDA_3          22\nSPMD0_1  SDDC_D0           23\nSPMD1_1  SDDC_D1           24\nSPMD2_1  SDDC_D2           25\nSPMD3_1  SDDC_D3           26\nSPMCK_1  SDDC_CK           27\nSPMCS0_1 SDDC_CMD          28\nSPMCS1_1                   29\n                           30\n                           31"
				(at -0.762 -3.048 0)
			)
			(pin bidirectional line
				(at -10.16 -6.35 0)
				(length 2.54)
				(name "PC0")
				(number "F9")
			)
			(pin bidirectional line
				(at -10.16 -8.89 0)
				(length 2.54)
				(name "PC1")
				(number "G9")
			)
			(pin bidirectional line
				(at -10.16 -11.43 0)
				(length 2.54)
				(name "PC2")
				(number "H9")
			)
			(pin bidirectional line
				(at -10.16 -13.97 0)
				(length 2.54)
				(name "PC3")
				(number "H8")
			)
			(pin bidirectional line
				(at -10.16 -16.51 0)
				(length 2.54)
				(name "PC4")
				(number "E8")
			)
			(pin bidirectional line
				(at -10.16 -19.05 0)
				(length 2.54)
				(name "PC5")
				(number "E3")
			)
			(pin bidirectional line
				(at -10.16 -21.59 0)
				(length 2.54)
				(name "PC6")
				(number "F4")
			)
			(pin bidirectional line
				(at -10.16 -24.13 0)
				(length 2.54)
				(name "PC7")
				(number "H7")
			)
			(pin bidirectional line
				(at -10.16 -26.67 0)
				(length 2.54)
				(name "PC8")
				(number "H6")
			)
			(pin bidirectional line
				(at -10.16 -29.21 0)
				(length 2.54)
				(name "PC9")
				(number "H3")
			)
			(pin bidirectional line
				(at -10.16 -31.75 0)
				(length 2.54)
				(name "PC10")
				(number "G1")
			)
			(pin bidirectional line
				(at -10.16 -34.29 0)
				(length 2.54)
				(name "PC11")
				(number "F1")
			)
			(pin bidirectional line
				(at -10.16 -36.83 0)
				(length 2.54)
				(name "PC12")
				(number "E1")
			)
			(pin bidirectional line
				(at -10.16 -39.37 0)
				(length 2.54)
				(name "PC13")
				(number "D1")
			)
			(pin bidirectional line
				(at -10.16 -41.91 0)
				(length 2.54)
				(name "PC14")
				(number "D2")
			)
			(pin bidirectional line
				(at -10.16 -44.45 0)
				(length 2.54)
				(name "PC15")
				(number "C2")
			)
		)
		(symbol "baochip1x_5_1"
			(text "GPIO"
				(at -7.112 -3.048 0)
			)
			(text "AF1      AF2      AF3      ANA\n\n\nKPI[0]\nKPI[1]\nKPI[2]\nKPI[3]\nKPO[0]\nKPO[1]            PWM0[2]*\nKPO[2]  I2CSDA_1* PWM0[1]*\nKPO[3]  I2CSCL_1* PWM0[0]*\n\nUARTRX_0          PWM0[3]\nUARTTX_0                   ADC0\n                  I2CSCL_0 ADC1\n                  I2CSDA_0 ADC2\n                           ADC3"
				(at 2.032 -3.048 0)
			)
			(text "* in bank PA"
				(at 8.128 -48.26 0)
			)
			(text "I/O level fixed to VDD33V rail"
				(at 19.304 -7.366 0)
			)
			(pin bidirectional line
				(at -10.16 -6.35 0)
				(length 2.54)
				(name "PF0")
				(number "E2")
			)
			(pin bidirectional line
				(at -10.16 -8.89 0)
				(length 2.54)
				(name "PF1")
				(number "E4")
			)
			(pin bidirectional line
				(at -10.16 -11.43 0)
				(length 2.54)
				(name "PF2")
				(number "G4")
			)
			(pin bidirectional line
				(at -10.16 -13.97 0)
				(length 2.54)
				(name "PF3")
				(number "G2")
			)
			(pin bidirectional line
				(at -10.16 -16.51 0)
				(length 2.54)
				(name "PF4")
				(number "G5")
			)
			(pin bidirectional line
				(at -10.16 -19.05 0)
				(length 2.54)
				(name "PF5")
				(number "G7")
			)
			(pin bidirectional line
				(at -10.16 -21.59 0)
				(length 2.54)
				(name "PF6")
				(number "G8")
			)
			(pin bidirectional line
				(at -10.16 -24.13 0)
				(length 2.54)
				(name "PF7_PA2")
				(number "F8")
			)
			(pin bidirectional line
				(at -10.16 -26.67 0)
				(length 2.54)
				(name "PF8_PA1")
				(number "F2")
			)
			(pin bidirectional line
				(at -10.16 -29.21 0)
				(length 2.54)
				(name "PF9_PA0")
				(number "C6")
			)
			(pin bidirectional line
				(at -10.16 -34.29 0)
				(length 2.54)
				(name "PA3")
				(number "F3")
			)
			(pin bidirectional line
				(at -10.16 -36.83 0)
				(length 2.54)
				(name "PA4")
				(number "G3")
			)
			(pin bidirectional line
				(at -10.16 -39.37 0)
				(length 2.54)
				(name "PA5")
				(number "C4")
			)
			(pin bidirectional line
				(at -10.16 -41.91 0)
				(length 2.54)
				(name "PA6")
				(number "F6")
			)
			(pin bidirectional line
				(at -10.16 -44.45 0)
				(length 2.54)
				(name "PA7")
				(number "D7")
			)
		)
		(embedded_fonts no)
	)
)
